Commission XIII : Fatigue of Welded components and structure (IIW 2017)

1)  XIII-2682-17 A comparison of fatigue performance between ferrite-pearlite and ferrite-bainite dual phase steels, D.G. Kim, J.Y. Park and M.H. Kim, Korea

2) XIII-2691-17 Fatigue strength of welded and HFMI-treated steel joints under constant and variable amplitude loading, M. Leitner, M. Ottersbock, S. Pubwald and H. Remes, Austria and Finland

3) XIII-2686-17 Fatigue assessment of the welded joints containing process relevant imperfection, E. Javaheri, K. Hemmesi, P. Tempel and M. Farajian, Germany

4) XIII-2702-17 2017 Report of work in progress on fatigue strength of welded joints in Japan, N. Osawa and E. Sakaki, Japan

5) XIII-2705-17 2017 report of work in progress in France, H-P. Lieurade, France

6) XIII-2687-17 Fatigue strength of thermal cut edges – Influence of ISO 9013 quality groups, P. Dieckhoff, J. Hensel, Th. Nitschke-Pagel and K. Dilger, Germany

7) XIII-2692-17 Fatigue strength of high-strength steel after shipyard production process of plasma cutting, grinding and sandblasting, I. Lillemae-Avi, S. Liinalampi, E. Lehtimaki, H. Remes. P. Lehto, J. Romanoff, S. Ehlers and A. Niemela, Finland and Germany

8) XIII-2700-17 Influence of welding heat input and welding residual stress on fracture parameter and fatigue crack propagation of a bead-on-plate specimen, R. Gadallah, N. Osawa and S. Tanaka, Japan

9) XIII-2684-17 Comparison of different numerical simulation approaches of high frequency mechanical impact (HFMI) treatment for optimization of the surface treatment process, C. Ernould, J. Schubnell, D. Simunek, M. Leitner, A. Maciolek, M. Farajian and M. Stoschka, Germany and Austria

10) XIII-2685-17 Reliable numerical and experimental characterization of residual stresses in multi- pass welds for high temperature applications, K. Hemmesi, M. Farajian, and M. Luke, Germany

11) XIII-2701-17 A study on corrosion fatigue and corrosion wastage in ship structures, N. Yamamoto, K. Ishibashi and T. Arima, Japan